**HK Audio SI SERIES**

**P10 rigging rail**

**Tender specifications**

Perforated rail for suspended mounting of speaker systems

Professional perforated rail for suspended mounting and precise alignment of up to three professional column speaker systems.

The perforated rail shall provide an easily accessible receptacle for typical rigging hardware (e.g., shackles, crimped wire rope brackets, etc.).

A separate anchor point must be included to brace the suspended loudspeakers, implement anti-rotation protection, or set the desired tilt angle.

**Technical data:**

Mounting type: suspended mounting

Functional description: simple mounting for suspended operation of up to three professional column speaker systems

Tilt range vertical: application-specific adjustable

Swivel range horizontal: application-specific adjustable

Material: steel

Surface: galvanized and smooth powder-coated (black, white or RAL according to requirements)

Dimensions (H x W x D): 146 x 128 x 217 mm

weight: 1.1 kg

**Lead product:**

The perforated rail for suspended mounting of speaker systems shall be the product **HK Audio SI SERIES P10 rigging rail.**