**HK Audio SI SERIES**

**P10 swivel and tilt bracket for one speaker**

**Tender specifications:**

Swivel and tilt bracketfor one speaker column system

Professional pan and tilt bracket for a speaker column system.

The bracket must be bolted to the back of the speaker system and be easy to operate and mount by simply hooking it into the wall bracket.

The maximum vertical tilt angle of the speaker mounted on it must be up to -18°. Likewise, a horizontal swiveling capability of the loudspeaker of up to 138° must be ensured.

**Technical data:**

Mounting type: wall mounting

Functional description: easy mounting by hanging and screwing; swiveling and tilting

Tilt range vertical: 0° to -18

Swivel range horizontal: 138°

Fixing points: 4x M6 for wall mounting

Material: steel

Surface: smooth powder coated (black, white or RAL according to requirements)

Dimensions (H x W x D): 160 x 90 x 106 mm

Weight: 1.1 kg

**Lead product:**

The swivel/tilt wall mount for a speaker column system shall be the product **HK Audio SI SERIES P10 swivel and tilt bracket for one speaker.**