**HK Audio SI SERIES**

**P10 Swivel and tilt bracket for two speakers**

**Tender specifications:**

Swivel and tilt bracket for two interconnected column speaker systems

Professional swivel and tilt bracket bracket for two column speaker systems.

The bracket must be bolted to the back of the speaker system and be easy to operate and mount by simply hooking it into the wall bracket.

The maximum vertical tilt angle of the speakers mounted on it must be up to -16°. Likewise, a horizontal swiveling of the speaker of up to 159° must be ensured.

**Technical data:**

Mounting type: wall mounting

Functional description: easy mounting by hanging and screwing; swiveling and tilting

Tilt range vertical: 0° to -16°

Swivel range horizontal: 159°

Mounting: 6x M6 for wall mounting

Material: steel

Surface: smooth powder-coated (black, white or RAL according to requirements)

Dimensions (H x W x D): 220 x 126 x 331 mm

weight: 2.9 kg

**Lead product:**

The swivel and tilt bracket for two column speaker systems shall be the product **HK Audio SI SERIES P10 swivel and tilt bracket for two speakers**.