**HK Audio SI SERIES S210 U-bracket**

**Tender specification**

**U-bracket for mounting speaker systems on walls, ceilings or for flown operation**

Professional U-bracket for mounting speaker systems on walls.

The U-bracket shall have slotted hole receptacles for M8 and smaller screws and shall also provide additional screw points for the attachment of screw-in hooks, e.g. for the purpose of cable routing.

The connection of the U-bracket to the loudspeaker housing must be designed with long-term stability using locking tooth lock washers.

The overall mechanism must be able to safely support one or two loudspeaker systems specified for this purpose, which must be demonstrated by testing and certification of ball impact resistance in accordance with DIN 18032-3.

Optional extension plates shall allow the secure mounting of the second speaker in each case.

**Technical data:**

Mounting method: wall mounting, ceiling mounting, flown installation.

Functional description: easy mounting by hanging and screwing; supports and swivels up to two speakers; certified ball impact resistance

Fasteners: 4x M8 mounting point, 4x M8 slotted hole, 2x M12 suspension point

Pivoting range: not provided

Material: steel

Surface: galvanized and smooth powder coated (black, white or RAL according to requirement)

Dimensions (H x W x D): 99 x 737 x 305 mm

Weight: 2.3 kg

**The bracket for mounting speaker systems on walls, ceilings or for flown operation shall be the product HK Audio SI SERIES S210 U-bracket.**