**HK Audio SI SERIES**

**P10 connector plate**

**Tender specifications:**

Connector plate for mechanical connection of several professional column speaker systems

Professional connector plate for mechanical connection of several professional column speaker systems.

The connector plates must be able to be screwed to the sides of the loudspeaker systems and must allow joint horizontal pivoting of several loudspeakers mounted one above the other.

**Technical data:**

Type of fastening: screw connection with loudspeaker housings

Functional description: mechanical connection of P10 loudspeaker enclosures

Material: steel

Surface: galvanized and smooth powder coated (black, white or RAL according to requirements)

dimensions (H x W x D): 211 x 90 x 2 mm

Weight: 0.25 kg

**Lead product:**

The connector plate for mechanical connection of several professional column speaker systems shall be the product **HK Audio SI SERIES P10 connector plate**.